Data Interpretation Practicum

Franklin Co. IN
1) Which soil map unit is considered to be prime farmland? See Franklin Doc#1--Farmland Classification?
A) CkC3
B) CkB2
C) Db
D) BoD2
E) EdG

2) Which soil map units are considered to have a high slippage potential?  See Franklin Doc#2—Soil Slippage Potential (see rating column in table)?
A) BrC3, BoD2
B) CbC2, CkC3
C) EbE2, EeD2
D) WeB2, RsB2
E) None of the above

3) Which soil map unit has loamy-skeletal alluvium as a parent material? See Franklin Doc#3—Parent Material Name?
A) Cm
B) RsA
C) AvA
D) Db
E) Both A & D

4) Which soil map units have a depth to a restrictive layer (fragipan) that are both <80cm? See Franklin Doc#4-Depth to a Soil Restrictive Layer-Fragipan?
A) RsA, RsB2
B) CkC3, RsB2
C) CkC3, CkB2
D) WeB2, EeD2
E) Cm, Db


Rio Arriba Area, NM
5) Bulk density data is used to compute available water capacity, total pore space, and other soil properties. The moist bulk density indicates pore space available for water and roots. Depending on soil texture, a bulk density of more than 1.4 can restrict water storage and root penetration. Which map unit is more than 1.4 grams/cm?
See Rio Arriba, NM_Doc#5 Bulk Density
A) Tinaja-Rock outcrop complex, 45-75% slopes
B) Menefee-Nalivag complex, 8-25% slopes
C) Menefee-Vesilla-Rock outcrop complex, 5 to 35% slopes 
D) None of the Above
E) All of the Above

6) [bookmark: _Hlk72918894]These soils have a low surface salinization risk:  See Rio Arriba, NM_ Doc#6 Surface Salts
A) [bookmark: _Hlk72919046][bookmark: _Hlk72919026]Menefee
B) Nalivag
C) Tinaja
D) None of the Above
E) All of the Above

7) For the mapunit 102-Menefee-Nalivag complex, 8 to 25 percent slopes, what is the Ecological Site Name of the Nalivag component?
See Rio Arriba, NM_Doc#7 - Ecological Sites
A) Loamy
B) Gravelly Fan
C) Gravelly-Woodland
D) Pinyan Upland
E) Steep Gravelly-Woodland

Delaware Co, NY 
8) If the client is concerned about potential flooding, which map unit would be the most Limiting for flooding? See Delaware, NY_Doc#8 - Flooding Frequency Class
A) Ff
B) Bs
C) Bg
D) Un
E) TkA



9) Which tree species are listed in the trees to manage column for the Bc map unit?  
See Delaware, NY_Doc#9_Forestland Productivity
A) Black walnut, eastern pine, white pine, Norway spruce
B) Black walnut, Eastern white pine, European larch, Norway spruce
C) Black walnut, Eastern white pine, Norway spruce
D) Douglas fir, European larch, Norway spruce, Red pine, White spruce
E) Eastern white pine, Norway spruce, Red pine

10) Which map unit is rated somewhat limited for disposal of wastewater by irrigation? 
See Delaware, NY_Doc#10– Wastewater by Irrigation
A) Ff
B) HcC
C) LkF
D) MaC
E) MaB

11) Which map unit has a farmland classification of “Farmland of statewide importance”? See Delaware, NY_Doc#11 – Farmland Classification
A) De
B) Nr
C) Pc
D) No
E) Ur

12) A client is interested in buying a piece of land with neutral pH soils. Which soil map units would have a Neutral pH range of 6.6-7.3? Pick the best answer.
See Delaware, NY_Doc# 12 – Health-Soil Reaction (pH)
A) Bc, Bg, Bs
B) ChC, ChD, ChE
C) MdC, MdB, OnB
D) MdB, MdC, MdD
E) OeA, OeB, OeC

Adams Co, IN
13) Which map unit has the highest percent (rating) for Organic Matter?
See Adams, IN_Doc #13-- Soil Health-Organic Matter
A) Pm
B) MsoA
C) Mh
D) BgmA
E) BgmB

Adams Co, IN #2

14) A client expresses an interest in a house site where they can have a basement. Which map unit would be most favorable for building a house with a basement?
 See Adams, IN_Doc  #14 – Dwelling with basements
A) Am
B) BleB
C) BgmB
D) RdB
E) GlsB

15) A builder is looking for a soil type that would have the least risk of corrosion to steel. Which soil type would have the least risk for this in building site development?
See Adams, IN_Doc #15 – Corrosion of Steel
A) RdB
B) HaA
C) BleA
D) GlsB
E) None of the above

16) Which components both fit into the Ecological Site Class of F111BY502IN – WET TILL RIDGE?  
See Adams, IN_Doc#16_Ecological Sites by Map Unit Component
A) Blount, Pewamo
B) Del Rey, Rawson
C) Blount, Haskins
D) Glynwood, Pewamo
E) Blount, Minster

17) Which map units all have a depth to water table greater than 23 cm?
See Adams, IN_Doc#17_Depth to Water Table
A) GlrB, GlsB, BleB
B) GlrB, GlsB, BgmB
C) GlrB, GlsB, HaA
D) GlrB, GlsB, BgmA
E) RdB, BgmB, GlrB



18) Which map units have a slope class of 2 to 6 percent? See Adams, IN_Doc#18_Soil Map
A) GlrB, GlsB, BleB
B) RdB, GlsB, BgmB
C) BgmB, BleB, RdB
D) GlrB, GlsB, RdB
E) BgmB, BleB, GlrB

19) Adams Co., IN has many soils with a dense restrictive layer (dense glacial till). Which map unit Will you NOT find a densic layer within 100 centimeters (under rating column) of the soil surface?
See Adams, IN_ Doc#19_Soil Features.
A) BgmA
B) Mh
C) BgmB
D) GlsB
E) None of the above

20) A wind erodibility group (WEG) consists of soils that have similar properties affecting the susceptibility to wind erosion in cultivated areas. The soils assigned to group 1 are the most susceptible to wind erosion, and those assigned to group 8 are the least susceptible. Which group of soils below are the most susceptible to wind erosion?
See Adams, IN_Doc#20_Wind Erodibility Group? Hint: look at rating column in the table.
A) Am, BgmA, GlsB
B) HaA, Mh, Pm
C) Am, Mh, Pm
D) GlrB, BleB, BleA
E) HaA, RdB, Pm
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